**Tillamook County**

DEPARTMENT OF COMMUNITY DEVELOPMENT

*BUILDING, PLANNING & ON-SITE SANITATION SECTIONS*

1510 - B Third St

Tillamook, OR 97141

503-842-3408

[www.tillamookcounty.gov](http://www.tillamookcounty.gov)

*Land of Cheese, Trees and Ocean Breeze*

SMOKE AND CARBON MONOXIDE ALARMS IN EACH SLEEPING ROOM CAN BE 2 SEPARATE DEVICES. IT’S OK TO LEAVE EXISTING SMOKE ALARMS AND INSTALL PLUG IN CARBON MONOXIDE DEVICES.

**Required Locations for Carbon Monoxide Alarms:**

1. In each sleeping room.
2. Within 15 feet outside each sleeping room door.

**Required Locations for Smoke Alarms:**

1. In each sleeping room.
2. Outside each separate sleeping area in the immediate vicinity of the bedrooms.
3. On each additional story of the dwelling, including basements and habitable attics and not including crawl spaces and uninhabitable attics. In dwellings or dwelling units with split levels and without an intervening door between the adjacent levels, a smoke alarm installed on the upper level shall suffice for the adjacent lower level provided that the lower level is less than one full story below the upper level.
4. Smoke alarms shall not be less than 3 feet horizontally from the door or opening of a bathroom that contains a bathtub or shower. Unless this would prevent placement of a smoke alarm required by this section.

**Required Locations for Smoke and Carbon Monoxide Alarms for Short-Term Rentals**





COMBINATION SMOKE AND CARBON MONOXIDE ALARMS CENTRALLY LOCATED IN CORRIDOR ARE ACCEPTABLE, BUT EXPENSIVE. AGAIN, 2 SEPARATE DEVICES ARE ACCEPTABLE AS WELL..